---
# SPDX-FileCopyrightText: Copyright (c) 2025-2026 NVIDIA CORPORATION & AFFILIATES. All rights reserved.
# SPDX-License-Identifier: Apache-2.0
title: vLLM-Omni
---

Dynamo supports multimodal generation through the [vLLM-Omni](https://github.com/vllm-project/vllm-omni) backend. This integration exposes text-to-text, text-to-image, and text-to-video capabilities via OpenAI-compatible API endpoints.

## Prerequisites

This guide assumes familiarity with deploying Dynamo with vLLM as described in the [vLLM backend guide](README.md).

### Installation

Dynamo container images include vLLM-Omni pre-installed. If you are using `pip install ai-dynamo[vllm]`, vLLM-Omni is **not** included automatically because the matching release is not yet available on PyPI. Install it separately from source:

```bash
pip install git+https://github.com/vllm-project/vllm-omni.git@v0.16.0rc1
```

## Supported Modalities

| Modality | Endpoint(s) | `--output-modalities` |
|---|---|---|
| Text-to-Text | `/v1/chat/completions` | `text` (default) |
| Text-to-Image | `/v1/chat/completions`, `/v1/images/generations` | `image` |
| Text-to-Video | `/v1/videos` | `video` |
| Image-to-Video | `/v1/videos` | `video` |

The `--output-modalities` flag determines which endpoint(s) the worker registers. When set to `image`, both `/v1/chat/completions` (returns inline base64 images) and `/v1/images/generations` are available. When set to `video`, the worker serves `/v1/videos`.

## Tested Models

| Modality | Models |
|---|---|
| Text-to-Text | `Qwen/Qwen2.5-Omni-7B` |
| Text-to-Image | `Qwen/Qwen-Image`, `AIDC-AI/Ovis-Image-7B` |
| Text-to-Video | `Wan-AI/Wan2.1-T2V-1.3B-Diffusers`, `Wan-AI/Wan2.2-T2V-A14B-Diffusers` |
| Image-to-Video | `Wan-AI/Wan2.2-TI2V-5B-Diffusers`, `Wan-AI/Wan2.2-I2V-A14B-Diffusers` |

To run a non-default model, pass `--model` to any launch script:

```bash
bash examples/backends/vllm/launch/agg_omni_image.sh --model AIDC-AI/Ovis-Image-7B
bash examples/backends/vllm/launch/agg_omni_video.sh --model Wan-AI/Wan2.2-T2V-A14B-Diffusers
```

## Text-to-Text

Launch an aggregated deployment (frontend + omni worker):

```bash
bash examples/backends/vllm/launch/agg_omni.sh
```

This starts `Qwen/Qwen2.5-Omni-7B` with a single-stage thinker config on one GPU.

Verify the deployment:

```bash
curl -s http://localhost:8000/v1/chat/completions \
  -H "Content-Type: application/json" \
  -d '{
    "model": "Qwen/Qwen2.5-Omni-7B",
    "messages": [{"role": "user", "content": "What is 2+2?"}],
    "max_tokens": 50,
    "stream": false
  }'
```

This script uses a custom stage config (`stage_configs/single_stage_llm.yaml`) that configures the thinker stage for text generation. See [Stage Configuration](#stage-configuration) for details.

## Text-to-Image

Launch using the provided script with `Qwen/Qwen-Image`:

```bash
bash examples/backends/vllm/launch/agg_omni_image.sh
```

### Via `/v1/chat/completions`

```bash
curl -s http://localhost:8000/v1/chat/completions \
  -H "Content-Type: application/json" \
  -d '{
    "model": "Qwen/Qwen-Image",
    "messages": [{"role": "user", "content": "A cat sitting on a windowsill"}],
    "stream": false
  }'
```

The response includes base64-encoded images inline:

```json
{
  "choices": [{
    "delta": {
      "content": [
        {"type": "image_url", "image_url": {"url": "data:image/png;base64,..."}}
      ]
    }
  }]
}
```

### Via `/v1/images/generations`

```bash
curl -s http://localhost:8000/v1/images/generations \
  -H "Content-Type: application/json" \
  -d '{
    "model": "Qwen/Qwen-Image",
    "prompt": "A cat sitting on a windowsill",
    "size": "1024x1024",
    "response_format": "url"
  }'
```

## Text-to-Video

Launch using the provided script with `Wan-AI/Wan2.1-T2V-1.3B-Diffusers`:

```bash
bash examples/backends/vllm/launch/agg_omni_video.sh
```

Generate a video via `/v1/videos`:

```bash
curl -s http://localhost:8000/v1/videos \
  -H "Content-Type: application/json" \
  -d '{
    "model": "Wan-AI/Wan2.1-T2V-1.3B-Diffusers",
    "prompt": "A drone flyover of a mountain landscape",
    "seconds": 2,
    "size": "832x480",
    "response_format": "url"
  }'
```

The response returns a video URL or base64 data depending on `response_format`:

```json
{
  "id": "...",
  "object": "video",
  "model": "Wan-AI/Wan2.1-T2V-1.3B-Diffusers",
  "status": "completed",
  "data": [{"url": "file:///tmp/dynamo_media/videos/req-abc123.mp4"}]
}
```

The `/v1/videos` endpoint also accepts NVIDIA extensions via the `nvext` field for fine-grained control:

| Field | Description | Default |
|---|---|---|
| `nvext.fps` | Frames per second | 24 |
| `nvext.num_frames` | Number of frames (overrides `fps * seconds`) | -- |
| `nvext.negative_prompt` | Negative prompt for guidance | -- |
| `nvext.num_inference_steps` | Number of denoising steps | 50 |
| `nvext.guidance_scale` | CFG guidance scale | 5.0 |
| `nvext.seed` | Random seed for reproducibility | -- |
| `nvext.boundary_ratio` | MoE expert switching boundary (I2V) | 0.875 |
| `nvext.guidance_scale_2` | CFG scale for low-noise expert (I2V) | 1.0 |

## Image-to-Video

Image-to-video (I2V) uses the same `/v1/videos` endpoint as text-to-video, with an additional `input_reference` field that provides the source image. The image can be an HTTP URL, a base64 data URI, or a local file path.

Launch with the provided script using `Wan-AI/Wan2.2-TI2V-5B-Diffusers`:

```bash
bash examples/backends/vllm/launch/agg_omni_i2v.sh
```

Generate a video from an image:

```bash
curl -s http://localhost:8000/v1/videos \
  -H "Content-Type: application/json" \
  -d '{
    "model": "Wan-AI/Wan2.2-TI2V-5B-Diffusers",
    "prompt": "A bear playing with yarn, smooth motion",
    "input_reference": "https://example.com/bear.png",
    "size": "832x480",
    "response_format": "url",
    "nvext": {
      "num_inference_steps": 40,
      "num_frames": 33,
      "guidance_scale": 1.0,
      "boundary_ratio": 0.875,
      "guidance_scale_2": 1.0,
      "seed": 42
    }
  }'
```

The `input_reference` field accepts:
- **HTTP/HTTPS URL**: `"https://example.com/image.png"`
- **Base64 data URI**: `"data:image/png;base64,iVBORw0KGgo..."`
- **Local file path**: `"/path/to/image.png"` or `"file:///path/to/image.png"`

The I2V-specific `nvext` fields (`boundary_ratio`, `guidance_scale_2`) control the dual-expert MoE denoising schedule in Wan2.x models. See [Wan2.2-I2V model card](https://huggingface.co/Wan-AI/Wan2.2-I2V-A14B-Diffusers) for details.

## CLI Reference

For the full list of Omni-related flags (including `--omni`, `--output-modalities`, `--stage-configs-path`, `--media-output-fs-url`, `--media-output-http-url`, and the `--omni-*` diffusion flags), run:

```bash
python -m dynamo.vllm --help
```

See also the [Argument Reference](vllm-reference-guide.md#argument-reference) in the Reference Guide.

## Storage Configuration

Generated images and videos are stored via [fsspec](https://filesystem-spec.readthedocs.io/), which supports local filesystems, S3, GCS, and Azure Blob.

By default, media is written to the local filesystem at `file:///tmp/dynamo_media`. To use cloud storage:

```bash
bash examples/backends/vllm/launch/agg_omni_video.sh \
  --media-output-fs-url s3://my-bucket/media \
  --media-output-http-url https://cdn.example.com/media
```

When `--media-output-http-url` is set, response URLs are rewritten as `{base-url}/{storage-path}` (e.g., `https://cdn.example.com/media/videos/req-id.mp4`). When unset, the raw filesystem path is returned.

For S3 credential configuration, set the standard AWS environment variables (`AWS_ACCESS_KEY_ID`, `AWS_SECRET_ACCESS_KEY`) or use IAM roles. See the [fsspec S3 docs](https://s3fs.readthedocs.io/en/latest/#credentials) for details.

## Stage Configuration

Omni pipelines are configured via YAML stage configs. See [`examples/backends/vllm/launch/stage_configs/single_stage_llm.yaml`](https://github.com/ai-dynamo/dynamo/blob/main/examples/backends/vllm/launch/stage_configs/single_stage_llm.yaml) for an example. For full documentation on stage config format and multi-stage pipelines, refer to the [vLLM-Omni Stage Configs documentation](https://docs.vllm.ai/projects/vllm-omni/en/latest/configuration/stage_configs/).

## Current Limitations

- Image input is supported only for I2V via `input_reference` in `/v1/videos`. Other endpoints accept text prompts only.
- KV cache events are not published for omni workers.
- Each worker supports a single output modality at a time.
