<!--
SPDX-FileCopyrightText: Copyright (c) 2025-2026 NVIDIA CORPORATION & AFFILIATES. All rights reserved.
SPDX-License-Identifier: Apache-2.0

Licensed under the Apache License, Version 2.0 (the "License");
you may not use this file except in compliance with the License.
You may obtain a copy of the License at

http://www.apache.org/licenses/LICENSE-2.0

Unless required by applicable law or agreed to in writing, software
distributed under the License is distributed on an "AS IS" BASIS,
WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
See the License for the specific language governing permissions and
limitations under the License.
-->

# dynamo.nixl_connect.WritableOperation

An operation which enables a remote worker to write data to the local worker.

To create the operation, a set of local [`Descriptor`](descriptor.md) objects must be provided which reference memory intended to receive data from a remote worker.
Once created, the memory referenced by the provided descriptors becomes immediately writable by a remote worker with the necessary metadata.
The NIXL metadata ([RdmaMetadata](rdma_metadata.md)) required to access the memory referenced by the provided descriptors is accessible via the operations `.metadata()` method.
Once acquired, the metadata needs to be provided to a remote worker via a secondary channel, most likely HTTP or TCP+NATS.

Disposal of the object will instruct the NIXL subsystem to cancel the operation,
therefore the operation should be awaited until completed unless cancellation is intended.
Cancellation is handled asynchronously.


## Example Usage

```python
    async def recv_data(
      self,
      local_tensor: torch.Tensor
    ) -> None:
      descriptor = dynamo.nixl_connect.Descriptor(local_tensor)

      with await self.connector.create_writable(descriptor) as write_op:
        op_metadata = write_op.metadata()

        # Send the metadata to the remote worker via sideband communication.
        await self.request_remote_data(op_metadata)
        # Wait the remote worker to complete its write operation to local_tensor.
        # AKA receive data from remote worker.
        await write_op.wait_for_completion()
```


## Methods

### `metadata`

```python
def metadata(self) -> RdmaMetadata:
```

Generates and returns the NIXL metadata ([RdmaMetadata](rdma_metadata.md)) required for a remote worker to write to the operation.
Once acquired, the metadata needs to be provided to a remote worker via a secondary channel, most likely HTTP or TCP+NATS.

### `wait_for_completion`

```python
async def wait_for_completion(self) -> None:
```

Blocks the caller until the operation has received a completion signal from a remote worker.


## Properties

### `status`

```python
@property
def status(self) -> OperationStatus:
```

Returns [`OperationStatus`](operation_status.md) which provides the current state (aka. status) of the operation.


## Related Classes

  - [Connector](connector.md)
  - [Descriptor](descriptor.md)
  - [Device](device.md)
  - [OperationStatus](operation_status.md)
  - [RdmaMetadata](rdma_metadata.md)
  - [ReadOperation](read_operation.md)
  - [ReadableOperation](readable_operation.md)
  - [WriteOperation](write_operation.md)
