(quantization-supported-hardware)=

# Supported Hardware

The table below shows the compatibility of various quantization implementations with different hardware platforms in vLLM:

:::{list-table}
:header-rows: 1
:widths: 20 8 8 8 8 8 8 8 8 8 8

- * Implementation
  * Volta
  * Turing
  * Ampere
  * Ada
  * Hopper
  * AMD GPU
  * Intel GPU
  * x86 CPU
  * AWS Inferentia
  * Google TPU
- * AWQ
  * ✗
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✅︎
  * ✅︎
  * ✗
  * ✗
- * GPTQ
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✅︎
  * ✅︎
  * ✗
  * ✗
- * Marlin (GPTQ/AWQ/FP8)
  * ✗
  * ✗
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✗
  * ✗
  * ✗
  * ✗
- * INT8 (W8A8)
  * ✗
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✗
  * ✅︎
  * ✗
  * ✗
- * FP8 (W8A8)
  * ✗
  * ✗
  * ✗
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✗
  * ✗
  * ✗
- * AQLM
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✗
  * ✗
  * ✗
  * ✗
- * bitsandbytes
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✗
  * ✗
  * ✗
  * ✗
- * DeepSpeedFP
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✗
  * ✗
  * ✗
  * ✗
- * GGUF
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✅︎
  * ✗
  * ✗
  * ✗
  * ✗

:::

- Volta refers to SM 7.0, Turing to SM 7.5, Ampere to SM 8.0/8.6, Ada to SM 8.9, and Hopper to SM 9.0.
- "✅︎" indicates that the quantization method is supported on the specified hardware.
- "✗" indicates that the quantization method is not supported on the specified hardware.

:::{note}
This compatibility chart is subject to change as vLLM continues to evolve and expand its support for different hardware platforms and quantization methods.

For the most up-to-date information on hardware support and quantization methods, please refer to <gh-dir:vllm/model_executor/layers/quantization> or consult with the vLLM development team.
:::
