[Back to supported operations](../../../include/ck/README.md)
# Composable Kernel Grouped Convolution

## Grouped Convolution Forward
Grouped convolution operation for 1D, 2D or 3D spatial dimensions. Convolution utilizes GEMM kernel after tensor coordinate transform. In CK Grouped Convolution Forward operation is called as `DeviceGroupedConvFwdMultipleABD` and requires following types as template parameters:

* **NumDimSpatial** - number of spatial dimensions (1D, 2D, 3D).
* **InLayout** - input layout (NHWGC, GNHWC, NGCHW).
* **WeiLayout** - weight layout (GKYXC).
* **DsLayout** - layouts for additional tensors for fused operations.
* **OutLayout** - output layout (NHWGK, GNHWK, NGKHW).
* **ADataType** - input data type. Pass tuple if there is fused operation with input.
* **BDataType** - weight data type. Pass tuple if there is fused operation with weight.
* **DsDataType** - data types for additional tensors for fused operations.
* **EDataType** - Output data type.
* **AElementwiseOperation** - fused operation on tensor A (input).
* **BElementwiseOperation** - fused operation on tensor B (weight).
* **CDEElementwiseOperation** - fused operation on tensor C (output).
* **AComputeType** - compute data type of tensor A for mfma instruction (ADataType by default).
* **BComputeType** - compute data type of tensor B for mfma instruction (AComputeType by default).

Grouped convolution forward support tensors larger than 2GB.

List of the device operations for grouped convolution forward in CK:

* **DeviceGroupedConvFwdMultipleABD_Xdl_CShuffle_V3** - Device operation with XDL instructions. Optimized for AMD Instinct MI300 series.
* **DeviceGroupedConvFwdMultipleABD_Xdl_CShuffle** - Device operation with XDL instructions and support of fused operations to input, weight and output.
* **DeviceGroupedConvFwdMultipleD_Wmma_CShuffle** - Device operation with WMMA instructions.
* **DeviceGroupedConvFwdDlMultipleD_NHWC_KYXC_NHWK** - Device operation with DL instructions.

Table of supported cases by instance factory with XDL instruction:

|       |NHWGC/GKYXC/NHWGK|NGCHW/GKYXC/NGKHW|GNHWC/GKYXC/GNHWK|
|-------|---|---|---|
|bf16 |2D, 3D|2D|1D, 2D, 3D|
|fp16 |2D, 3D|2D|1D, 2D, 3D|
|fp32 |2D, 3D|2D|1D, 2D, 3D|
|int8 |2D, 3D|2D|1D, 3D|
|fp8  |3D|&cross;|&cross;|
|bf8  |3D|&cross;|&cross;|

Table of supported cases by instance factory with WMMA instruction:

|       |NHWGC/GKYXC/NHWGK|NGCHW/GKYXC/NGKHW|GNHWC/GKYXC/GNHWK|
|-------|---|---|---|
|fp16 |2D, 3D|&cross;|2D, 3D|
|int8 |2D, 3D|&cross;|2D, 3D|

Table of supported cases by instance factory with DL instruction:

|       |NHWGC/GKYXC/NHWGK|NGCHW/GKYXC/NGKHW|GNHWC/GKYXC/GNHWK|
|-------|---|---|---|
|bf16 |&cross;|&cross;|2D|
|fp16 |&cross;|&cross;|2D|
|fp32 |&cross;|&cross;|2D|
|int8 |&cross;|&cross;|2D|

Table of supported cases by instance factory with fused elementwise operation:

* **Dynamic elementwise operation** - 2D/3D, NHWGC, bf16/fp16/fp32/int8
* **Bilinear** - 3D, NHWGC, bf16/fp16/fp32/int8
* **ConvInvScale** - 3D, NHWGC, fp8
* **ConvScale** - 3D, NHWGC, fp8/bf8
* **ConvScale + Add** - 3D, NHWGC, fp8
* **ConvScale + Relu** - 3D, NHWGC, fp8
* **Scale** - 3D, NHWGC, bf16/fp16/fp32/int8
* **Scale + Add (for A and B)** - 3D, NHWGC, bf16/fp16/fp32/int8
* **Scale + Add + Scale + Add + Relu** - 3D, NHWGC, bf16/fp16/fp32/int8
