# Qwen3.6
## 论文
[Qwen3.6](https://qwen.ai/blog?id=qwen3.6)

## 模型简介

Qwen3.6-35B-A3B 是一款采用混合专家 (MoE) 架构并包含视觉编码器的多模态因果语言模型。总参数量为 35B，推理时激活参数量为 3B。此版本重点优化了智能体编程 (Agentic Coding) 的准确率，并引入了思维保留 (Thinking Preservation) 机制，特别适合长上下文和复杂的代码仓库开发任务。

<div align=center>
    <img src="./doc/qwen3.5_397b_a17b_infra.jpg"/>
</div>

## 环境依赖
| 软件 |                    版本                     |
| :------: |:-----------------------------------------:|
| DTK |                   26.04                   |
| python |                  3.10.12                  |
| transformers |            5.5.0               |
| vllm |      0.18.1+das.3266200.dtk2604     |
| triton |      3.4.0+git1ef59765      |
| torch |   2.10.0+das.opt1.dtk2604.20260325.g6b060a   |

当前仅支持定制镜像: harbor.sourcefind.cn:5443/dcu/admin/base/custom:vllm018-ubuntu22.04-dtk26.04-gemma4-0413

- 挂载地址`-v` 根据实际模型情况修改
```bash
docker run -it \
    --shm-size 200g \
    --network=host \
    --name qwen3.5 \
    --privileged \
    --device=/dev/kfd \
    --device=/dev/dri \
    --device=/dev/mkfd \
    --group-add video \
    --cap-add=SYS_PTRACE \
    --security-opt seccomp=unconfined \
    -u root \
    -v /opt/hyhal/:/opt/hyhal/:ro \
    -v /path/your_code_data/:/path/your_code_data/ \
    harbor.sourcefind.cn:5443/dcu/admin/base/custom:vllm018-ubuntu22.04-dtk26.04-gemma4-0413 bash
```
更多镜像可前往[光源](https://sourcefind.cn/#/service-list)下载使用。

关于本项目DCU显卡所需的特殊深度学习库可从[光合](https://developer.sourcefind.cn/tool/)开发者社区下载安装。

## 数据集
暂无

## 训练
暂无

## 推理
> 如果出现`ImportError: librocm_smi64.so.2: cannot open shaned object file: No such file or directory`报错，系机器hyhal版本较低所致，请进行升级。

### vllm
**mtp**功能需添加以下参数：
```
--speculative-config.method mtp  \
--speculative-config.num_speculative_tokens 2
```

#### 单机推理
```bash
## serve启动
vllm serve Qwen/Qwen3.5-35B-A3B \
    --port 8001 \
    --trust-remote-code \
    --dtype bfloat16 \
    --tensor-parallel-size 2 \
    --gpu-memory-utilization 0.925 \
    --default-chat-template-kwargs '{"enable_thinking": false}' \
    --reasoning-parser qwen3 \
    --enable-auto-tool-choice \
    --tool-call-parser qwen3_coder

## client访问
curl http://localhost:8001/v1/chat/completions   \
    -H "Content-Type: application/json"  \
    -d '{
        "model": "Qwen/Qwen3.5-35B-A3B",
        "messages": [
          {"role": "user", "content": "Type \"I love Qwen3.5\" backwards"}
        ],
        "temperature": 0.6
    }'
```

#### 多机推理
1. 加入环境变量
> 请注意：
> 每个节点上的环境变量都写到.sh文件中，保存后各个计算节点分别source`.sh`文件
>
> VLLM_HOST_IP：节点本地通信口ip，尽量选择IB网卡的IP，**避免出现rccl超时问题**
>
> NCCL_SOCKET_IFNAME和 GLOO_SOCKET_IFNAME：节点本地通信网口ip对应的名称
>
> 通信口和ip查询方法：ifconfig
>
> IB口状态查询：ibstat  !!!一定要active激活状态才可用，各个节点要保持统一

```bash
export ALLREDUCE_STREAM_WITH_COMPUTE=1
export VLLM_HOST_IP=x.x.x.x # 对应计算节点的IP，选择IB口SOCKET_IFNAME对应IP地址
export NCCL_SOCKET_IFNAME=ibxxxx
export GLOO_SOCKET_IFNAME=ibxxxx
export NCCL_IB_HCA=mlx5_x:1 # 环境中的IB网卡名字
unset NCCL_ALGO
export NCCL_MIN_NCHANNELS=16
export NCCL_MAX_NCHANNELS=16
export NCCL_NET_GDR_READ=1
export HIP_VISIBLE_DEVICES=0,1,2,3,4,5,6,7
export VLLM_RPC_TIMEOUT=1800000

# 海光CPU绑定核
export VLLM_NUMA_BIND=1
export VLLM_RANK0_NUMA=0
export VLLM_RANK1_NUMA=1
export VLLM_RANK2_NUMA=2
export VLLM_RANK3_NUMA=3
export VLLM_RANK4_NUMA=4
export VLLM_RANK5_NUMA=5
export VLLM_RANK6_NUMA=6
export VLLM_RANK7_NUMA=7
```

2. 启动RAY集群
> x.x.x.x 对应第一步 VLLM_HOST_IP

```bash
# head节点执行
ray start --head --node-ip-address=x.x.x.x --port=6379 --num-gpus=8 --num-cpus=32
# worker节点执行
ray start --address='x.x.x.x:6379' --num-gpus=8 --num-cpus=32
```

3. 启动vllm server
```bash
## serve启动
vllm serve Qwen/Qwen3.5-397B-A17B \
    --port 8001 \
    --tensor-parallel-size 16 \
    --distributed-executor-backend ray \
    --trust-remote-code \
    --dtype bfloat16 \
    --gpu-memory-utilization 0.925 \
    --default-chat-template-kwargs '{"enable_thinking": false}' \
    --reasoning-parser qwen3 \
    --enable-auto-tool-choice \
    --tool-call-parser qwen3_coder

## client访问
curl http://localhost:8001/v1/chat/completions   \
    -H "Content-Type: application/json"  \
    -d '{
        "model": "Qwen/Qwen3.5-397B-A17B",
        "messages": [
          {"role": "user", "content": "Type \"I love Qwen3.5\" backwards"}
        ],
        "temperature": 0.6
    }'
```

## 效果展示
<div align=center>
    <img src="./doc/result-dcu.jpg"/>
</div>

### 精度
DCU与GPU精度一致，推理框架：vllm。

## 预训练权重
|  模型名称  | 权重大小 | DCU型号  | 最低卡数需求 |         下载地址          |
|:------:|:----:|:----------:|:------:|:---------------------:|
| Qwen3.5-397B-A17B | 397B | K100AI,BW1000 |   16   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-397B-A17B) |
| Qwen3.5-397B-A17B-INT8 | 397B | BW1000 |   8   | [Modelscope](https://www.modelscope.cn/models/metax-tech/Qwen3.5-397B-A17B-W8A8) |
| Qwen3.5-122B-A10B | 122B | K100AI,BW1000 |   8   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-122B-A10B) |
| Qwen3.5-35B-A3B | 35B | K100AI,BW1000 |   2   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-35B-A3B) |
| Qwen3.5-27B | 27B | K100AI,BW1000 |   2   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-27B) |
| Qwen3.5-9B | 9B | K100AI,BW1000 |   1   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-9B) |
| Qwen3.5-4B | 4B | K100AI,BW1000 |   1   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-4B) |
| Qwen3.5-2B | 2B | K100AI,BW1000 |   1   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-2B) |
| Qwen3.5-0.8B | 0.8B | K100AI,BW1000 |   1   | [Hugging Face](https://huggingface.co/Qwen/Qwen3.5-0.8B) |

## 源码仓库及问题反馈
- https://developer.sourcefind.cn/codes/modelzoo/qwen3.5_vllm

## 参考资料
- https://github.com/QwenLM/Qwen3.5
