diff --git a/ggml-metal.m b/ggml-metal.m
index 0207b787..b5e9884b 100644
--- a/ggml-metal.m
+++ b/ggml-metal.m
@@ -1396,27 +1396,23 @@ static enum ggml_status ggml_metal_graph_compute(
                         // to the matrix-vector kernel
                         int ne11_mm_min = 1;
 
-#if 0
                         // the numbers below are measured on M2 Ultra for 7B and 13B models
                         // these numbers do not translate to other devices or model sizes
                         // TODO: need to find a better approach
-                        if ([ctx->device.name isEqualToString:@"Apple M2 Ultra"]) {
-                            switch (src0t) {
-                                case GGML_TYPE_F16:  ne11_mm_min = 2;  break;
-                                case GGML_TYPE_Q8_0: ne11_mm_min = 7;  break;
-                                case GGML_TYPE_Q2_K: ne11_mm_min = 15; break;
-                                case GGML_TYPE_Q3_K: ne11_mm_min = 7;  break;
-                                case GGML_TYPE_Q4_0:
-                                case GGML_TYPE_Q4_1: ne11_mm_min = 15; break;
-                                case GGML_TYPE_Q4_K: ne11_mm_min = 11; break;
-                                case GGML_TYPE_Q5_0:                          // not tested yet
-                                case GGML_TYPE_Q5_1: ne11_mm_min = 13; break; // not tested yet
-                                case GGML_TYPE_Q5_K: ne11_mm_min = 7;  break;
-                                case GGML_TYPE_Q6_K: ne11_mm_min = 7;  break;
-                                default:             ne11_mm_min = 1;  break;
-                            }
+                        switch (src0t) {
+                            case GGML_TYPE_F16:  ne11_mm_min = 2;  break;
+                            case GGML_TYPE_Q8_0: ne11_mm_min = 7;  break;
+                            case GGML_TYPE_Q2_K: ne11_mm_min = 15; break;
+                            case GGML_TYPE_Q3_K: ne11_mm_min = 7;  break;
+                            case GGML_TYPE_Q4_0:
+                            case GGML_TYPE_Q4_1: ne11_mm_min = 15; break;
+                            case GGML_TYPE_Q4_K: ne11_mm_min = 11; break;
+                            case GGML_TYPE_Q5_0:                          // not tested yet
+                            case GGML_TYPE_Q5_1: ne11_mm_min = 13; break; // not tested yet
+                            case GGML_TYPE_Q5_K: ne11_mm_min = 7;  break;
+                            case GGML_TYPE_Q6_K: ne11_mm_min = 7;  break;
+                            default:             ne11_mm_min = 1;  break;
                         }
-#endif
 
                         // for now the matrix-matrix multiplication kernel only works on A14+/M1+ SoCs
                         // AMD GPU and older A-chips will reuse matrix-vector multiplication kernel
