---
id: pr-sglang-23620
repo: sgl-project/sglang
pr: 23620
title: '[AMD] Optimize MiniMax-M2.5 - enable fused Triton kernel for FP8 KV cache write in aiter decode path'
author: yctseng0211
date: '2026-04-25'
url: https://github.com/sgl-project/sglang/pull/23620
source_category: upstream-code
architectures:
- sm100
tags: []
techniques: []
hardware_features: []
kernel_types: []
languages: []
captured_at: '2026-05-16'
status: merged
merge_sha: adc59325bc67f6ed2dcf0c95863387402000326f
inclusion_reason: defer
changed_paths:
- python/sglang/srt/layers/attention/aiter_backend.py
artifact_dir: evidence/pull-bundles/sglang/gh-23620
head_ref_oid: e56aec7da3096e5028c74ccafdccc64f75978972
---
# [AMD] Optimize MiniMax-M2.5 - enable fused Triton kernel for FP8 KV cache write in aiter decode path

- Repository: `sgl-project/sglang`
- PR: [23620](https://github.com/sgl-project/sglang/pull/23620)
- Decision: `defer`
- Reason: defer

## Changed Paths

- `python/sglang/srt/layers/attention/aiter_backend.py`

## Evidence Bundle

`evidence/pull-bundles/sglang/gh-23620`
