---
id: pr-vllm-23642
repo: vllm-project/vllm
pr: 23642
title: '[Model] Use the same fused_moe configs for all H200 devices'
author: bufferoverflow
date: '2025-10-30'
url: https://github.com/vllm-project/vllm/pull/23642
source_category: upstream-code
architectures:
- sm100
tags: []
techniques: []
hardware_features: []
kernel_types: []
languages: []
captured_at: '2026-05-16'
status: merged
merge_sha: 2918c1b49c88c29783c86f78d2c4221cb9622379
inclusion_reason: defer
changed_paths:
- vllm/model_executor/layers/fused_moe/fused_moe.py
artifact_dir: evidence/pull-bundles/vllm/gh-23642
head_ref_oid: 737005bf65770112712ce861120e5549a096aa23
---
# [Model] Use the same fused_moe configs for all H200 devices

- Repository: `vllm-project/vllm`
- PR: [23642](https://github.com/vllm-project/vllm/pull/23642)
- Decision: `defer`
- Reason: defer

## Changed Paths

- `vllm/model_executor/layers/fused_moe/fused_moe.py`

## Evidence Bundle

`evidence/pull-bundles/vllm/gh-23642`
