<!--
SPDX-FileCopyrightText: Copyright (c) 2025 NVIDIA CORPORATION & AFFILIATES. All rights reserved.
SPDX-License-Identifier: Apache-2.0

Licensed under the Apache License, Version 2.0 (the "License");
you may not use this file except in compliance with the License.
You may obtain a copy of the License at

http://www.apache.org/licenses/LICENSE-2.0

Unless required by applicable law or agreed to in writing, software
distributed under the License is distributed on an "AS IS" BASIS,
WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
See the License for the specific language governing permissions and
limitations under the License.
-->

# Dynamo Distributed Runtime

## Overview

Dynamo `DistributedRuntime` is the core infrastructure in dynamo that enables distributed communication and coordination between different dynamo components. It is implemented in rust (`/lib/runtime`) and exposed to other programming languages via binding (i.e., python bindings can be found in `/lib/bindings/python`). `DistributedRuntime` follows a hierarchical structure:

- `DistributedRuntime`: This is the highest level object that exposes the distributed runtime interface. It maintains connection to external services (e.g., etcd for service discovery and NATS for messaging) and manages lifecycle with cancellation tokens.
- `Namespace`: A `Namespace` is a logical grouping of components that isolate between different model deployments.
- `Component`: A `Component` is a discoverable object within a `Namespace` that represents a logical unit of workers.
- `Endpoint`: An `Endpoint` is a network-accessible service that provides a specific service or function.

While theoretically each `DistributedRuntime` can have multiple `Namespace`s as long as their names are unique (similar logic also applies to `Component/Namespace` and `Endpoint/Component`), in practice, each dynamo components typically are deployed with its own process and thus has its own `DistributedRuntime` object. However, they share the same namespace to discover each other.

For example, the deployment configuration `examples/llm/configs/disagg.yaml` have four workers:

- `Frontend`: Start an HTTP server and register a `chat/completions` endpoint. The HTTP server route the request to the `Processor`.
- `Processor`: When a new request arrives, `Processor` applies the chat template and perform the tokenization. Then, it route the request to the `VllmWorker`.
- `VllmWorker` and `PrefillWorker`: Perform the actual decode and prefill computation.

Since the four workers are deployed in different processes, each of them have their own `DistributedRuntime`. Within their own `DistributedRuntime`, they all have their own `Namespace`s named `dynamo`. Then, under their own `dynamo` namespace, they have their own `Component`s named `Frontend/Processor/VllmWorker/PrefillWorker`. Lastly, for the `Endpoint`, `Frontend` has no `Endpoints`, `Processor` and `VllmWorker` each has a `generate` endpoint, and `PrefillWorker` has a placeholder `mock` endpoint.

## Initialization

In this section, we explain what happens under the hood when `DistributedRuntime/Namespace/Component/Endpoint` objects are created. There are two modes for `DistributedRuntime` initialization: dynamic and static. In static mode, components and endpoints are defined using known addresses and do not change during runtime. In dynamic modes, components and endpoints are discovered through the network and can change during runtime. We focus on the dynamic mode in the rest of this document. Static mode is basically dynamic mode without registration and discovery and hence does not rely on etcd.

```{caution}
The hierarchy and naming in etcd and NATS may change over time, and this document might not reflect the latest changes. Regardless of such changes, the main concepts would remain the same.
```

- `DistributedRuntime`: When a `DistributedRuntime` object is created, it establishes connections to the following two services:
    - etcd (dynamic mode only): for service discovery. In static mode, `DistributedRuntime` can operate without etcd.
    - NATS (both static and dynamic mode): for messaging.

  where etcd and NATS are two global services (there could be multiple etcd and NATS services for high availability).

  For etcd, it also creates a primary lease and spin up a background task to keep the lease alive. All objects registered under this `DistributedRuntime` use this lease_id to maintain their life cycle. There is also a cancellation token that is tied to the primary lease. When the cancellation token is triggered or the background task failed, the primary lease is revoked or expired and the kv pairs stored with this lease_id is removed.
- `Namespace`: `Namespace`s are primarily a logical grouping mechanism and is not registered in etcd. It provides the root path for all components under this `Namespace`.
- `Component`: When a `Component` object is created, similar to `Namespace`, it isn't be registered in etcd. When `create_service` is called, it creates a NATS service group using `{namespace_name}.{service_name}` and registers a service in the registry of the `Component`, where the registry is an internal data structure that tracks all services and endpoints within the `DistributedRuntime`.
- `Endpoint`: When an Endpoint object is created and started, it performs two key registrations:
  - NATS Registration: The endpoint is registered with the NATS service group created during service creation. The endpoint is assigned a unique subject following the naming: `{namespace_name}.{service_name}.{endpoint_name}-{lease_id_hex}`.
  - etcd Registration: The endpoint information is stored in etcd at a path following the naming: `/services/{namespace}/{component}/{endpoint}-{lease_id}`. Note that the endpoints of different workers of the same type (i.e., two `PrefillWorker`s in one deployment) share the same `Namespace`, `Componenet`, and `Endpoint` name. They are distinguished by their different primary `lease_id` of their `DistributedRuntime`.

## Calling Endpoints

Dynamo uses `Client` object to call an endpoint. When a `Client` objected is created, it is given the name of the `Namespace`, `Component`, and `Endpoint`. It then sets up an etcd watcher to monitor the prefix `/services/{namespace}/{component}/{endpoint}`. The etcd watcher continuously updates the `Client` with the information, including `lease_id` and NATS subject of the available `Endpoint`s.

The user can decide which load balancing strategy to use when calling the `Endpoint` from the `Client`, which is done in [push_router.rs](../../lib/runtime/src/pipeline/network/egress/push_router.rs). Dynamo supports three load balancing strategies:

- `random`: randomly select an endpoint to hit
- `round_robin`: select endpoints in round-robin order
- `direct`: direct the request to a specific endpoint by specifying the `lease_id` of the endpoint

After selecting which endpoint to hit, the `Client` sends the serialized request to the NATS subject of the selected `Endpoint`. The `Endpoint` receives the request and create a TCP response stream using the connection information from the request, which establishes a direct TCP connection to the `Client`. Then, as the worker generates the response, it serializes each response chunk and sends the serialized data over the TCP connection.

## Examples

We provide native rust and python (through binding) examples for basic usage of `DistributedRuntime`:

- Rust: `/lib/runtime/examples/`
- Python: `/lib/bindings/python/examples/`. We also provide a complete example of using `DistributedRuntime` for communication and Dynamo's LLM library for prompt templates and (de)tokenization to deploy a vllm-based service. Please refer to `lib/bindings/python/examples/hello_world/server_vllm.py` for details.

```{note}
Building a vLLM docker image for ARM machines currently involves building vLLM from source, which is known to be slow and requires extensive system RAM; see [vLLM Issue 8878](https://github.com/vllm-project/vllm/issues/8878).

You can tune the number of parallel build jobs for building VLLM from source
on ARM based on your available cores and system RAM with `VLLM_MAX_JOBS`.

For example, on an ARM machine with low system resources:
`./container/build.sh --framework vllm --platform linux/arm64 --build-arg VLLM_MAX_JOBS=2`

For example, on a GB200 which has very high CPU cores and memory resource:
`./container/build.sh --framework vllm --platform linux/arm64 --build-arg VLLM_MAX_JOBS=64`

When vLLM has pre-built ARM wheels published, this process can be improved.
```
